,Wattage Comments[-1010500]##OTHER##,Wattage[-1150103]##ELECTRICAL_WATTAGE##WATTS,Voltage Loss[-1150110]##OTHER##,URL[-1010104]##OTHER##,Type Comments[-1010105]##OTHER##,Total Light Loss Factor[-1114217]##OTHER##,Tilt Angle[-1010505]##ANGLE##DEGREES,Temperature Loss[-1150109]##OTHER##,Temperature Color[-1150134]##OTHER##,Surface Depreciation Loss[-1150113]##OTHER##,Photometric Web File[-1140034]##OTHER##,None[-1150142]##OTHER##,Model[-1010109]##OTHER##,Manufacturer[-1010108]##OTHER##,Luminous Flux[-1010503]##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation[-1150115]##OTHER##,Luminous Intensity[-1150105]##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Light Loss Input Method[-1150137]##OTHER##,Lamp Tilt Loss[-1150112]##OTHER##,Lamp Lumen Depreciation[-1150114]##OTHER##,Lamp[-1010501]##OTHER##,Initial Light Intensity Input Method[-1150132]##OTHER##,Initial Color Temperature[-1150107]##COLOR_TEMPERATURE##KELVIN,Illuminance[-1150106]##ELECTRICAL_ILLUMINANCE##LUX,IES Files Link##OTHER##,Emit from Line Length[-1150126]##LENGTH##FEET,Efficacy[-1150104]##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift[-1150117]##OTHER##,Description[-1010103]##OTHER##,Default Elevation[-1154647]##LENGTH##FEET,Color Filter[-1150108]##OTHER##,Ballast Loss[-1114218]##OTHER##,At a distance[-1150133]##LENGTH##FEET
4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(2000L),20W,19.999195818255,1,https://iuseelite.com/product/4-fpl2-bl-led-ml-cct/,4ft,1,90.000000000000,1,0,1,4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(2000L).IES,"",4-FPL2-BL-LED-ML-CCT,Elite Lighting,2486.900000000000,1,818.240000000000,0,1,1,LED,2,3500.000000000000,88.074620593686,https://media.iuseelite.com/ies/4-fpl2-bl-led-ml-cct.zip,2.000000000000,124.350000000000,0,4 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000
4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(3000L),30W,29.999139118457,1,https://iuseelite.com/product/4-fpl2-bl-led-ml-cct/,4ft,1,90.000000000000,1,0,1,4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(3000L).IES,,4-FPL2-BL-LED-ML-CCT,Elite Lighting,3484.700000000000,1,1134.610000000000,0,1,1,LED,2,3500.000000000000,122.128403979030,https://media.iuseelite.com/ies/4-fpl2-bl-led-ml-cct.zip,2.000000000000,116.160000000000,0,4 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000
4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(4000L),40W,40.000000000000,1,https://iuseelite.com/product/4-fpl2-bl-led-ml-cct/,4ft,1,90.000000000000,1,0,1,4-FPL2-BL-LED-3ML-DIM10-MVOLT-5CCT-85(4000L).IES,,4-FPL2-BL-LED-ML-CCT,Elite Lighting,4497.200000000000,1,1483.800000000000,0,1,1,LED,2,3500.000000000000,159.714902763139,https://media.iuseelite.com/ies/4-fpl2-bl-led-ml-cct.zip,2.000000000000,112.430000000000,0,4 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000