,Wattage Comments[-1010500]##OTHER##,Wattage[-1150103]##ELECTRICAL_WATTAGE##WATTS,Voltage Loss[-1150110]##OTHER##,URL[-1010104]##OTHER##,Type Comments[-1010105]##OTHER##,Total Light Loss Factor[-1114217]##OTHER##,Tilt Angle[-1010505]##ANGLE##DEGREES,Temperature Loss[-1150109]##OTHER##,Temperature Color[-1150134]##OTHER##,Surface Depreciation Loss[-1150113]##OTHER##,Photometric Web File[-1140034]##OTHER##,None[-1150142]##OTHER##,Model[-1010109]##OTHER##,Manufacturer[-1010108]##OTHER##,Luminous Flux[-1010503]##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation[-1150115]##OTHER##,Luminous Intensity[-1150105]##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Light Loss Input Method[-1150137]##OTHER##,Lamp Tilt Loss[-1150112]##OTHER##,Lamp Lumen Depreciation[-1150114]##OTHER##,Lamp[-1010501]##OTHER##,Initial Light Intensity Input Method[-1150132]##OTHER##,Initial Color Temperature[-1150107]##COLOR_TEMPERATURE##KELVIN,Illuminance[-1150106]##ELECTRICAL_ILLUMINANCE##LUX,IES Files Link##OTHER##,Emit from Line Length[-1150126]##LENGTH##FEET,Efficacy[-1150104]##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift[-1150117]##OTHER##,Description[-1010103]##OTHER##,Default Elevation[-1154647]##LENGTH##FEET,Color Filter[-1150108]##OTHER##,Ballast Loss[-1114218]##OTHER##,At a distance[-1150133]##LENGTH##FEET
2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(1000L),15W,15.000000000000,1,https://iuseelite.com/product/2-fpl2-bl-led-ml-cct/,2ft,1,90.000000000000,1,0,1,2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(1000L).IES,"",2-FPL2-BL-LED-ML-CCT,Elite Lighting,1689.000000000000,1,561.680000000000,0,1,1,LED,2,3500.000000000000,60.458732028575,https://media.iuseelite.com/ies/2-fpl2-bl-led-ml-cct.zip,2.000000000000,112.600000000000,0,2 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000
2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(1500L),17W,17.000261073884,1,https://iuseelite.com/product/2-fpl2-bl-led-ml-cct/,2ft,1,90.000000000000,1,0,1,2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(1500L).IES,"",2-FPL2-BL-LED-ML-CCT,Elite Lighting,1953.500000000000,1,646.920000000000,0,1,1,LED,2,3500.000000000000,69.633889267779,https://media.iuseelite.com/ies/2-fpl2-bl-led-ml-cct.zip,2.000000000000,114.910000000000,0,2 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000
2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(2000L),20W,19.999101769514,1,https://iuseelite.com/product/2-fpl2-bl-led-ml-cct/,2ft,1,90.000000000000,1,0,1,2-FPL2-BL-LED-3ML-DIM10-MVOLT-4CCT-85(2000L).IES,"",2-FPL2-BL-LED-ML-CCT,Elite Lighting,2226.500000000000,1,737.710000000000,0,1,1,LED,2,3500.000000000000,79.406443535109,https://media.iuseelite.com/ies/2-fpl2-bl-led-ml-cct.zip,2.000000000000,111.330000000000,0,2 ft Slim LED Linear Panel Series with Multi-CCT,0.000000000000,16777215,1,10.000000000000